TRIBIT STORMBOX LAVA PORTABLE WIRELESS SPEAKER
Accessible User Guide (English)
TRIBIT StormBox Lava Portable Wireless Speaker
Model: BTS51
What’s in the Box
· StormBox Lava Portable Wireless Speaker
· USB-C Charging Cable
· USB-A Output Port
· Carrying Straps
· User Documentation
Button Press Definitions
These symbols describe how to press any referenced button:
· x1 = Press once
· x2 = Press twice
· x3 = Press three times
· 2S = Press and hold for 2 seconds
· Reset = Hold the + and – buttons together for 5 seconds
Charging the Speaker
· When the battery is below 20 percent, a red light blinks.
· While charging, the red light stays on.
· When fully charged (about 5 hours), the red light turns off.
Note: Keep the charging port and cable completely dry while charging.
Charging Other Devices
You can charge external devices using the speaker’s USB-A port. The speaker will stop charging other devices if its own battery drops below 20 percent.
Power On and Off
· Press the Power button (x1) to turn the speaker on or off.
· If there is no audio or any button activity, the speaker will automatically turn off after 75 minutes.
· To force a shutdown, press and hold the Power button (2S), then restart the speaker.
Pairing (Bluetooth)
· Press the Bluetooth button (x1) to enter pairing mode.
· Press and hold the Bluetooth button (2S) to disconnect the Bluetooth connection.
· The speaker can connect to up to two Bluetooth devices at the same time.
Note: If Bluetooth and a wired AUX connection are both active, press the Bluetooth button (x2) to switch between them.
Button Layout (Left to Right)
· Power Button
· Bluetooth Button
· Minus Button (Volume Down)
· Multifunction Circle Button (Play / Pause)
· Plus Button (Volume Up)
· XBass Button
· TWS Button (Stereo Mode and Party Mode)
Stereo Mode (TWS)
You can pair two StormBox Lava speakers into a Left and Right stereo pair.
1. Connect Speaker A to your phone’s Bluetooth.
2. Make sure Speaker B is not connected to any device.
3. Press the TWS button (x1) on both speakers.
4. Once paired: 
· Speaker A becomes the left channel.
· Speaker B becomes the right channel.
5. To exit Stereo Mode, press and hold the TWS button (2S) on either speaker.
Party Mode (Up to 100+ Speakers)
You can link multiple StormBox Lava speakers for synchronized playback.
1. Connect the host speaker A to your phone’s Bluetooth.
2. Press the TWS button (x2) on the host speaker.
3. Make sure all other speakers are not connected to any device.
4. Press the TWS button (x2) on each additional speaker.
5. Each speaker will announce when it successfully joins the group.
6. Up to 100+ speakers can play together.
7. To exit Party Mode, press and hold the TWS button (2S) on any speaker.
Tribit App
Use the Tribit app to:
· Adjust EQ settings
· Update firmware
· Access additional features
Safety Precautions
· Ensure the silicone plug on the charging port is tightly closed before exposure to water.
· Keep the charging port and cable completely dry during charging.
· Do not drop the speaker or place it where it can fall.
· Do not disassemble, modify, or attempt to repair the speaker.
· This product contains a lithium battery. Do not burn or expose it to excessive heat.
· Use a power adapter that meets local safety standards.
· Warranty period: 12 months.
Specifications
· Bluetooth Version: V5.4
· Output Power: 80W total (30W × 2 woofers, 10W × 2 tweeters)
· Bluetooth Protocols: A2DP, AVRCP, HFP, HSP
· Frequency Response: 43Hz to 20kHz
· Frequency Band: 2402 to 2480MHz
· Maximum Transmission Power: ≤ 6 dBm
· Battery Capacity: 43.2Wh
· Play Time: Up to 24 hours (50 percent volume, XBass Off)
· Charging Time: About 5 hours with a 15W charger
· Waterproof Rating: IP67
· Dimensions: 310mm × 147mm × 152mm
· Dimensions (inches): 12.2 × 5.8 × 6.0
· Weight: 2300g (5.07 lbs)
FCC Statement
This device complies with Part 15 of the FCC Rules. Operation is subject to:
1. This device may not cause harmful interference.
2. This device must accept any interference received, including interference that may cause undesired operation.
If interference occurs:
· Reorient or relocate the receiving antenna.
· Increase separation between the equipment and receiver.
· Connect the device to a different circuit.
· Consult a radio or TV technician.
Unauthorized modifications may void FCC authorization.
IC Statement (Canada)
This device complies with Industry Canada licence-exempt RSS standards. Operation is subject to:
1. This device may not cause interference.
2. This device must accept any interference received, including interference that may cause undesired operation.
Support Information
· For proper charging, use a power adapter between 2W and 15W.
· Compliance documents cover multiple Tribit models, including BTS51.

